Configuration	test
STM32CubeMX 	6.12.0
Date	02/05/2026
MCU	STM32F103CBTx



PERIPHERALS	MODES	FUNCTIONS	PINS
RCC	Crystal/Ceramic Resonator	RCC_OSC_IN	PD0-OSC_IN
RCC	Crystal/Ceramic Resonator	RCC_OSC_OUT	PD1-OSC_OUT
SYS	Serial Wire	SYS_JTCK-SWCLK	PA14
SYS	Serial Wire	SYS_JTMS-SWDIO	PA13
SYS	SysTick	SYS_VS_Systick	VP_SYS_VS_Systick
TIM2	Internal Clock	TIM2_VS_ClockSourceINT	VP_TIM2_VS_ClockSourceINT
TIM2	Output Compare CH1	TIM2_CH1	PA0-WKUP



Pin Nb	PINs	FUNCTIONs	LABELs
5	PD0-OSC_IN	RCC_OSC_IN	
6	PD1-OSC_OUT	RCC_OSC_OUT	
10	PA0-WKUP	TIM2_CH1	
11	PA1	GPIO_Input	B0
12	PA2	GPIO_Input	B1
13	PA3	GPIO_Input	B2
14	PA4	GPIO_Input	B3
15	PA5	GPIO_Input	B4
16	PA6	GPIO_Input	B5
17	PA7	GPIO_Input	B6
18	PB0	GPIO_Output	LED0
19	PB1	GPIO_Output	LED1
20	PB2	GPIO_Output	LED2
21	PB10	GPIO_Output	PCDA2
22	PB11	GPIO_Output	PCDA3
25	PB12	GPIO_Output	PCDA4
26	PB13	GPIO_Output	PCDA5
27	PB14	GPIO_Output	PCDA6
28	PB15	GPIO_Output	PCDA7
29	PA8	GPIO_Input	B7
30	PA9	GPIO_Input	PRG
34	PA13	SYS_JTMS-SWDIO	
37	PA14	SYS_JTCK-SWCLK	
39	PB3	GPIO_Output	LED3
40	PB4	GPIO_Output	LED4
41	PB5	GPIO_Output	LED5
42	PB6	GPIO_Output	LED6
43	PB7	GPIO_Output	LED7
45	PB8	GPIO_Output	PCDA0
46	PB9	GPIO_Output	PCDA1
PERIPHERALS	MODES	FUNCTIONS	PINS
RCC	Crystal/Ceramic Resonator	RCC_OSC_IN	PD0-OSC_IN
RCC	Crystal/Ceramic Resonator	RCC_OSC_OUT	PD1-OSC_OUT
SYS	Serial Wire	SYS_JTCK-SWCLK	PA14
SYS	Serial Wire	SYS_JTMS-SWDIO	PA13
SYS	SysTick	SYS_VS_Systick	VP_SYS_VS_Systick
TIM2	Internal Clock	TIM2_VS_ClockSourceINT	VP_TIM2_VS_ClockSourceINT
TIM2	Output Compare CH1	TIM2_CH1	PA0-WKUP



Pin Nb	PINs	FUNCTIONs	LABELs
5	PD0-OSC_IN	RCC_OSC_IN	
6	PD1-OSC_OUT	RCC_OSC_OUT	
10	PA0-WKUP	TIM2_CH1	
11	PA1	GPIO_Input	B0
12	PA2	GPIO_Input	B1
13	PA3	GPIO_Input	B2
14	PA4	GPIO_Input	B3
15	PA5	GPIO_Input	B4
16	PA6	GPIO_Input	B5
17	PA7	GPIO_Input	B6
18	PB0	GPIO_Output	LED0
19	PB1	GPIO_Output	LED1
20	PB2	GPIO_Output	LED2
21	PB10	GPIO_Output	PCDA2
22	PB11	GPIO_Output	PCDA3
25	PB12	GPIO_Output	PCDA4
26	PB13	GPIO_Output	PCDA5
27	PB14	GPIO_Output	PCDA6
28	PB15	GPIO_Output	PCDA7
29	PA8	GPIO_Input	B7
30	PA9	GPIO_Input	PRG
34	PA13	SYS_JTMS-SWDIO	
37	PA14	SYS_JTCK-SWCLK	
39	PB3	GPIO_Output	LED3
40	PB4	GPIO_Output	LED4
41	PB5	GPIO_Output	LED5
42	PB6	GPIO_Output	LED6
43	PB7	GPIO_Output	LED7
45	PB8	GPIO_Output	PCDA0
46	PB9	GPIO_Output	PCDA1



SOFTWARE PROJECT

Project Settings : 
Project Name : test
Project Folder : C:\Users\PC_home_2\STM32CubeIDE\workspace_1.16.0\test
Toolchain / IDE : STM32CubeIDE
Firmware Package Name and Version : STM32Cube FW_F1 V1.8.6


Code Generation Settings : 
STM32Cube MCU packages and embedded software packs : Copy only the necessary library files
Generate peripheral initialization as a pair of '.c/.h' files per peripheral : No
Backup previously generated files when re-generating : No
Delete previously generated files when not re-generated : Yes
Set all free pins as analog (to optimize the power consumption) : No


Toolchains Settings : 
Compiler Optimizations : 





